**QUOTATION OF WL825T WHEEL LOADER**

Delivery time: About 80 working days upon receipt of deposit

Warranty: 12 months

Packing: 2 sets WL825T+1x WE18 in 1\*40HQ (WE18 need to dismantle boom)

Price List

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | **Picture** | **Standard Configurations** | **DAP Price (EUR)** |
| **WL825T** |  | Changchai 4G33 engine 70kw, electronic control joystick , LED lights, back camera, Varta Battery, 16/70-20 tires, luxury cabin with heater, 220V engine preheat, warning light, adjustable steering wheel and seat, radio, fan, hand brake, extinguisher, Free parts, tool box. | **€28900** |

Option Configuration

|  |  |  |  |
| --- | --- | --- | --- |
| Yunnei DEF20CAF4 E5 55kw | + € 4800 | FOTON CUMMINS QSF2.84TC74 | +€8000 |
| Kohler KDI2504 EPA4 E5 55kw | + € 8500 | DF Cummins 4BT3.9-C100 | +€6500 |
| Xinchai 4E30yg40 E5 55.8kw | + €5000 | Change to fully electronic control | +€700 |
| Extra oil cooler | +€450 | Diesel heater | +€600 |
| Add 4th electric switch | + €300 | Air conditioning | +€600 |
| Quick hitch | + €500 |  |  |

Attachments

|  |  |  |  |
| --- | --- | --- | --- |
| Pallet fork | €700 | Grass fork | €1200 |
| Hydraulic adjustable pallet fork | €1300 | Snow bucket | €1200 |
| Snow blade with spring 2.1m | €1200 | Auger | €1700 |
| V Blade | €1100 | Bale spear(2&3 teeth) | €800 |
| 4 in 1 bucket | €1150 | Open Sweeper | €1350 |
| Drum clamp | €780 | Closed street sweeper | €2500 |
| digger arm (Backhoe bucket) | €1100 | Log clamp (H model) | €1200 |
| Dustpan bucket | €700 | Screening bucket | €750 |
| Lifting arm | €1120 | grass cutter | €1120 |
| Pitch fork | €980 | New European grass fork | €980 |
| Bale grab | €1120 | Grab bucket | €1500 |

|  |  |  |
| --- | --- | --- |
| Whole drive system | Hydraulic system(torque converter) | |
| Specification | Overall weight(kg) | 5700 |
| L×W×H（mm） | 6000×2100×2580 |
| Rated bucket capacity(m3) | 0.8-0.9 |
| Rated load(kg) | 2000 |
| Max Load (kg) | 2500 |
| Dump height (mm) | 4200 |
| Dump distance(mm) | 510 |
| Wheel base(mm) | 1550 |
| Thread(mm) | 2550 |
| Total time(s) | 8 |
| Engine | Model | Changchai4G33 engine |
| Type | Direct injection, Horizontal, Water-cooled, Four stroke |
| Rated power（KW） | 70 |
| Rated speed(r/min) | 2400 |
| Working system | Gearbox type | ZL-15 |
| Walking pump | ZK-18 |
| Working pump (Double Pump) | CBQL-F2063 |
| Steering system | Max. turning angle | 45 |
| Min turning radius(mm) | 4300 |
| Hydraulic system | Working pressure | 16Mpa |
| Boom lifting time | 4.8S |
| Tank capacity | 70L |
| Tires | Standard tires | 16/70-20 |
| Stand bucket | Width (mm) | 2100 |

Specifications

Pictures

|  |  |
| --- | --- |
| 3 |  |
| GG3G8644 | GG3G8701 |
| 2 | 1 |
| Fajl_011-1-scaled | Fajl_000-6-scaled |
|  | IMG_8799 |

