**QUOTATION OF MINI750 WHEEL LOADER**

Delivery time: About 80 working days upon receipt of deposit

Warranty: 12 months

Packing: 3 sets/20GP; 7 sets/40HQ

Price List

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | **Picture** | **Standard Configurations** | **DAP Price (EUR)** |
| **Mini750T**  **With cabin** |  | Perkins 403J-11 E5/EPA engine, 18.4kw  PWG Italy hydraulic system;  26x1200-12 wider tires, electric joystick, Quick hitch included, standard bucket, VARTA Battery, floating function.Standard with 3 hydraulic lines | **21900** |

Option Configuration

|  |  |
| --- | --- |
| **Option** | **Price（USD）** |
| Kubota D1105 Euro5/EPA4 18.2 | +$700 |
| Fully electronic joystick | +$800 |
| With canopy | -$350 |
| 27x8.5-15 narrow tire | Same price |

Attachments

|  |  |  |  |
| --- | --- | --- | --- |
| Pallet fork | € 570 | Grass fork | €1100 |
| Hydraulic adjustable pallet fork | € 1450 | Snow bucket | €1000 |
| Snow blade with spring | €1300 | Auger | €1500 |
| V Blade | €1000 | Bale spear(2&3 teeth) | €1100 |
| 4 in 1 bucket | €1000 | Open Sweeper | €1400 |
| Drum clamp | €1000 | Closed street sweeper | €1800 |
| digger arm (Backhoe bucket) | €1500 | Log clamp (H model/A model) | €1350 |
| No tooth bucket | €400 | Screening bucket | €660 |
| Dustpan bucket | €900 | Grass bucket | €960 |
| Lifting arm | €1200 | New European grass fork | €1220 |
| Pitch fork | €980 | Bale grab | €1100 |
| Grass cutter | €1350 |  |  |

|  |  |
| --- | --- |
| **Standard Engine** | |
| Model | Perkins 403J-11 Euro V |
| Rated power | 18.4 kw |
| Rated speed | 2200rpm |
| Maximum torque | 67Nm |
| **Dimensions** | |
| Overall Size LxWxH | 3882x1150x2275mm |
| Minimum ground clearance | 355mm |
| Maximum dumping height | 2475mm |
| Dumping reach | 893mm |
| Wheel base | 1340mm |
| **Performance parameters of the machine** | |
| Bucket | 0.2-0.4m3 |
| Tipping load in shovel, vehicle straight | 798kg |
| Tipping load in shovel, vehicle at 68° | 498kg |
| Operating weight | 2050kg |
| The sum of the work device | 7.5s |
| Driving speed | 0-12km/h |
| **Minimum turning-circle radius** | |
| Outside face of bucket | 2411mm |
| Outside face of tyre | 2060mm |
| Tire Model | 26\*12-12 |
| Maximum turning angle | ±47.78° |

Specifications

Pictures

|  |  |
| --- | --- |
|  |  |
|  |  |
| 微信图片_202306131050204 | 微信图片_20231130164537 |

